For the road, we will make it 3 mm in height, railroad style. Each railroad tie will also be 3 mm in height, but also 2 mm in width. Run with gaps also in 3 mm.

Main arch will be in two parts per side. Full arch is 300 mm in length, and 100 mm in height. Beam thickness is

Makerbot Cloud Print

<https://cloudprint.makerbot.com/print>